Atari800Win Plus: Monitor Commands

CONT 				- Continue emulation 
SHOW 				- Show registers 
STACK 				- Show stack 
SET<PC,A,S,X,Y> hexval 		- Set register value
SET<N,V,D,I,Z,C> 			- Set flag value
CLR<N,V,D,I,Z,C> 			- Clear flag value
C startaddr hexval... 			- Change memory
D [startaddr] 				- Disassemble memory
F startaddr endaddr hexval 		- Fill memory
M [startaddr] 			- Memory list
S startaddr endaddr hexval... 	- Search memory
ROM startaddr endaddr 		- Convert memory block into ROM
RAM startaddr endaddr 		- Convert memory block into RAM
HARDWARE startaddr endaddr 	- Convert memory block into HARDWARE
READ filename start addr nbytes 	- Read file into memory
WRITE startaddr endaddr [file] 	- Write memory block to a file <memdump.dat>
SUM startaddr endaddr 		- SUM of specified memory range
TRON file 				- Trace on
TROFF 				- Trace off
BREAK [addr] 			- Set breakpoint at address
YBREAK [pos] , or [l000+pos] 	- Break at scanline or flash scanline
BRK on: off 				- Set BRK opcode behavior
HISTORY or H 			- Disasm. last 128 PC addrs. giving ypos xpos 
JUMPS 				- List last 32 locations of JMP/JSR
G 					- Execute 1 instruction 
O					- Step over the instruction
R					- Execute until return 
B					- Breakpoint <B ? for help>  
A [startaddr]				- Start simple assembler
ANTIC, GTIA, PIA, POKEY	- Display hardware registers
DLIST [startaddr]			- Show Display List 
PROFILE				- Display profiling statistics 
LABELS file 				- Load labels from file <xasm format>
COLDSTART, WARMSTART	- Perform system coldstart / warmstart
! command				- Execute shell command
QUIT					- Quit emulator
EXIT					- Exit emulator
HELP or ? 				- This text